(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "AllConnectBaseboard:VIO" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 3.81 -1.27 0))
      (property "Value" "VIO" (id 1) (at 0 2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VIO\"" (id 5) (at 0 0 0))
      (symbol "VIO_0_0"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VIO")
          (number "1")
        )
      )
      (symbol "VIO_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
    )
    (symbol "Connector:Conn_01x03_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0))
      (property "Value" "Conn_01x03_Male" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x03_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
      )
    )
    (symbol "Device:C_Polarized_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Polarized_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "C_Polarized_Small_0_1"
        (rectangle (start -1.524 -0.3048) (end 1.524 -0.6858)
          (fill (type outline))
        )
        (rectangle (start -1.524 0.6858) (end 1.524 0.3048)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.524)
            (xy -0.762 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.27)
            (xy -1.016 1.778)
          )
          (fill (type none))
        )
      )
      (symbol "C_Polarized_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 1.8542)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.8542)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Ferrite" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at -1.27 0 90))
      (property "Value" "L_Ferrite" (id 1) (at 2.794 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor with ferrite core" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_Ferrite_0_1"
        (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -2.794)
            (xy 1.016 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -1.778)
            (xy 1.016 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -0.762)
            (xy 1.016 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0.254)
            (xy 1.016 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 1.016 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 2.286)
            (xy 1.016 2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -2.286)
            (xy 1.524 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -1.27)
            (xy 1.524 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -0.254)
            (xy 1.524 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 0.762)
            (xy 1.524 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 1.778)
            (xy 1.524 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 2.794)
            (xy 1.524 2.286)
          )
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_Ferrite_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:SM6T6V8A" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "SM6T6V8A" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_SMD:D_SMB" (id 2) (at 0 -5.08 0))
      (property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf" (id 3) (at -1.27 0 0))
      (property "ki_keywords" "diode TVS voltage suppressor" (id 4) (at 0 0 0))
      (property "ki_description" "600W unidirectional Transil Transient Voltage Suppressor, 6.8Vrwm, DO-214AA" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*SMB*" (id 6) (at 0 0 0))
      (symbol "SM6T6V8A_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "SM6T6V8A_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
      )
    )
    (symbol "Regulator_Switching:AP63200WU" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 6.35 0))
      (property "Value" "AP63200WU" (id 1) (at 2.54 6.35 0))
      (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6" (id 2) (at 0 -22.86 0))
      (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP63200-AP63201-AP63203-AP63205.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "2A Buck DC/DC" (id 4) (at 0 0 0))
      (property "ki_description" "2A, 500kHz Buck DC/DC Converter, adjustable output voltage, TSOT-23-6" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TSOT?23*" (id 6) (at 0 0 0))
      (symbol "AP63200WU_0_1"
        (rectangle (start -7.62 5.08) (end 7.62 -5.08)
          (fill (type background))
        )
      )
      (symbol "AP63200WU_1_1"
        (pin input line (at 10.16 -2.54 180) (length 2.54)
          (name "FB")
          (number "1")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "EN")
          (number "2")
        )
        (pin power_in line (at -10.16 2.54 0) (length 2.54)
          (name "IN")
          (number "3")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin output line (at 10.16 2.54 180) (length 2.54)
          (name "SW")
          (number "5")
        )
        (pin passive line (at 10.16 0 180) (length 2.54)
          (name "BST")
          (number "6")
        )
      )
    )
    (symbol "power:+24V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+24V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "global power" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+24V\"" (id 5) (at 0 0 0))
      (symbol "+24V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+24V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+24V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 183.515 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 111.125 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 120.015 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 208.915 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 213.995 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 90.805 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 196.215 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 165.735 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 183.515 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 196.215 91.44) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 123.825 86.36) (xy 120.015 86.36)))
  (wire (pts (xy 111.125 88.9) (xy 111.125 93.98)))
  (wire (pts (xy 150.495 81.28) (xy 150.495 76.2)))
  (wire (pts (xy 196.215 90.17) (xy 196.215 91.44)))
  (wire (pts (xy 217.805 95.25) (xy 208.915 95.25)))
  (wire (pts (xy 217.805 97.79) (xy 217.805 95.25)))
  (wire (pts (xy 213.995 81.28) (xy 213.995 83.82)))
  (wire (pts (xy 90.805 77.47) (xy 90.805 81.28)))
  (wire (pts (xy 212.725 107.95) (xy 212.725 105.41)))
  (wire (pts (xy 111.125 81.28) (xy 111.125 83.82)))
  (wire (pts (xy 196.215 83.82) (xy 213.995 83.82)))
  (wire (pts (xy 208.915 95.25) (xy 208.915 91.44)))
  (wire (pts (xy 217.805 107.95) (xy 217.805 102.87)))
  (wire (pts (xy 170.815 83.82) (xy 165.735 83.82)))
  (wire (pts (xy 149.225 86.36) (xy 149.225 91.44)))
  (wire (pts (xy 215.265 107.95) (xy 217.805 107.95)))
  (wire (pts (xy 149.225 91.44) (xy 183.515 91.44)))
  (wire (pts (xy 183.515 90.17) (xy 183.515 91.44)))
  (wire (pts (xy 196.215 96.52) (xy 196.215 97.79)))
  (wire (pts (xy 90.805 81.28) (xy 90.805 82.55)))
  (wire (pts (xy 208.915 102.87) (xy 208.915 107.95)))
  (wire (pts (xy 111.125 81.28) (xy 120.015 81.28)))
  (wire (pts (xy 183.515 83.82) (xy 196.215 83.82)))
  (wire (pts (xy 120.015 86.36) (xy 120.015 81.28)))
  (wire (pts (xy 196.215 83.82) (xy 196.215 85.09)))
  (wire (pts (xy 183.515 83.82) (xy 183.515 85.09)))
  (wire (pts (xy 208.915 97.79) (xy 208.915 95.25)))
  (wire (pts (xy 208.915 107.95) (xy 210.185 107.95)))
  (wire (pts (xy 165.735 76.2) (xy 165.735 83.82)))
  (wire (pts (xy 90.805 90.17) (xy 90.805 93.98)))
  (wire (pts (xy 120.015 81.28) (xy 123.825 81.28)))
  (wire (pts (xy 178.435 83.82) (xy 183.515 83.82)))
  (wire (pts (xy 144.145 81.28) (xy 150.495 81.28)))
  (wire (pts (xy 144.145 83.82) (xy 154.305 83.82)))
  (wire (pts (xy 150.495 76.2) (xy 165.735 76.2)))
  (wire (pts (xy 90.805 81.28) (xy 111.125 81.28)))
  (wire (pts (xy 159.385 83.82) (xy 165.735 83.82)))
  (wire (pts (xy 144.145 86.36) (xy 149.225 86.36)))
  (wire (pts (xy 208.915 91.44) (xy 196.215 91.44)))
  (wire (pts (xy 183.515 91.44) (xy 196.215 91.44)))
  (text "Selectable 12V / 5V / 3.3V supply" (at 99.695 67.31 0))
  (text "12V" (at 220.345 106.68 90))
  (text "32V_{in,max}" (at 122.555 91.44 0))
  (text "5V" (at 208.915 106.68 90))
  (text "Jumper selectability:\nNo jumper: 3.3V\nJumper [1] & [2] - 5V\nJumper [2] & [3] - 12V\n\nNo possibility of bad jumpering"
    (at 200.66 128.905 0)
  )
  (symbol (lib_id "Regulator_Switching:AP63200WU") (at 133.985 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 133.985 73.025 0))
    (property "Value" "AP63200WU" (id 1) (at 133.985 75.565 0))
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6" (id 2) (at 133.985 106.68 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP63200-AP63201-AP63203-AP63205.pdf" (id 3) (at 133.985 83.82 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Device:R_Small") (at 217.805 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R4" (id 0) (at 220.345 99.0599 0))
    (property "Value" "20k" (id 1) (at 220.345 101.5999 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 217.805 100.33 0))
    (property "Datasheet" "~" (id 3) (at 217.805 100.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 156.845 83.82 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 158.115 82.55 90))
    (property "Value" "100nF 25V" (id 1) (at 151.765 80.01 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 156.845 83.82 0))
    (property "Datasheet" "~" (id 3) (at 156.845 83.82 0))
    (property "MPN" "CL10B104KB8NNWC" (id 4) (at 156.845 83.82 0))
    (property "MPNA1" "CL10B104KB8NNNC" (id 5) (at 156.845 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+24V") (at 90.805 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 90.805 81.28 0))
    (property "Value" "+24V" (id 1) (at 90.805 72.39 0))
    (property "Footprint" "" (id 2) (at 90.805 77.47 0))
    (property "Datasheet" "" (id 3) (at 90.805 77.47 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 196.215 87.63 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R1" (id 0) (at 198.755 86.3599 0))
    (property "Value" "220k" (id 1) (at 198.755 88.8999 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 196.215 87.63 0))
    (property "Datasheet" "~" (id 3) (at 196.215 87.63 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "AllConnectBaseboard:VIO") (at 213.995 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR07" (id 0) (at 217.805 82.55 0))
    (property "Value" "VIO" (id 1) (at 213.995 76.2 0))
    (property "Footprint" "" (id 2) (at 213.995 81.28 0))
    (property "Datasheet" "" (id 3) (at 213.995 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:SM6T6V8A") (at 90.805 86.36 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D1" (id 0) (at 93.98 85.0899 90))
    (property "Value" "SMAJ24A" (id 1) (at 93.98 87.6299 90))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 85.725 86.36 0))
    (property "Datasheet" "" (id 3) (at 90.805 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Ferrite") (at 174.625 83.82 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L1" (id 0) (at 174.625 76.835 90))
    (property "Value" "10uH 2A" (id 1) (at 174.625 79.375 90))
    (property "Footprint" "Inductor_SMD:L_Taiyo-Yuden_NR-50xx" (id 2) (at 174.625 83.82 0))
    (property "Datasheet" "~" (id 3) (at 174.625 83.82 0))
    (property "MPN" "NRS5040T100MMGJ" (id 4) (at 174.625 83.82 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized_Small") (at 111.125 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 111.76 83.82 0))
    (property "Value" "47uF 35V" (id 1) (at 111.76 88.9 0))
    (property "Footprint" "Capacitor_SMD:CP_Elec_6.3x5.4" (id 2) (at 111.125 86.36 0))
    (property "Datasheet" "~" (id 3) (at 111.125 86.36 0))
    (property "MPN" "RVT47UF35V67RV0039" (id 4) (at 111.125 86.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 111.125 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR03" (id 0) (at 111.125 100.33 0))
    (property "Value" "GND" (id 1) (at 111.125 98.425 0))
    (property "Footprint" "" (id 2) (at 111.125 93.98 0))
    (property "Datasheet" "" (id 3) (at 111.125 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:Conn_01x03_Male") (at 212.725 113.03 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 207.645 112.395 90))
    (property "Value" "Conn_01x03_Male" (id 1) (at 207.645 112.395 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (id 2) (at 212.725 113.03 0))
    (property "Datasheet" "~" (id 3) (at 212.725 113.03 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:GND") (at 90.805 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR02" (id 0) (at 90.805 100.33 0))
    (property "Value" "GND" (id 1) (at 90.805 98.425 0))
    (property "Footprint" "" (id 2) (at 90.805 93.98 0))
    (property "Datasheet" "" (id 3) (at 90.805 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 212.725 105.41 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR06" (id 0) (at 212.725 99.06 0))
    (property "Value" "GND" (id 1) (at 212.7249 101.6 90))
    (property "Footprint" "" (id 2) (at 212.725 105.41 0))
    (property "Datasheet" "" (id 3) (at 212.725 105.41 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 208.915 100.33 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R3" (id 0) (at 202.565 100.33 90))
    (property "Value" "110k" (id 1) (at 205.105 100.33 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 208.915 100.33 0))
    (property "Datasheet" "~" (id 3) (at 208.915 100.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized_Small") (at 213.995 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C4" (id 0) (at 216.535 84.5438 0))
    (property "Value" "47uF 35V" (id 1) (at 216.535 87.0838 0))
    (property "Footprint" "Capacitor_SMD:CP_Elec_6.3x5.4" (id 2) (at 213.995 86.36 0))
    (property "Datasheet" "~" (id 3) (at 213.995 86.36 0))
    (property "MPN" "RVT47UF35V67RV0039" (id 4) (at 213.995 86.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 213.995 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR08" (id 0) (at 213.995 95.25 0))
    (property "Value" "GND" (id 1) (at 213.995 93.345 0))
    (property "Footprint" "" (id 2) (at 213.995 88.9 0))
    (property "Datasheet" "" (id 3) (at 213.995 88.9 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 133.985 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR04" (id 0) (at 133.985 97.79 0))
    (property "Value" "GND" (id 1) (at 133.985 95.885 0))
    (property "Footprint" "" (id 2) (at 133.985 91.44 0))
    (property "Datasheet" "" (id 3) (at 133.985 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 196.215 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R2" (id 0) (at 198.755 92.7099 0))
    (property "Value" "68k" (id 1) (at 198.755 95.2499 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 196.215 93.98 0))
    (property "Datasheet" "~" (id 3) (at 196.215 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 183.515 87.63 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C3" (id 0) (at 186.055 86.3662 0))
    (property "Value" "100pF" (id 1) (at 186.055 88.9062 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 183.515 87.63 0))
    (property "Datasheet" "~" (id 3) (at 183.515 87.63 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 196.215 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR05" (id 0) (at 196.215 104.14 0))
    (property "Value" "GND" (id 1) (at 196.215 102.87 0))
    (property "Footprint" "" (id 2) (at 196.215 97.79 0))
    (property "Datasheet" "" (id 3) (at 196.215 97.79 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR02") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "VIO") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+24V") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "47uF 35V") (footprint "Capacitor_SMD:CP_Elec_6.3x5.4")
    )
    (path
      (reference "C2") (unit 1) (value "100nF 25V") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C3") (unit 1) (value "100pF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C4") (unit 1) (value "47uF 35V") (footprint "Capacitor_SMD:CP_Elec_6.3x5.4")
    )
    (path
      (reference "D1") (unit 1) (value "SMAJ24A") (footprint "Diode_SMD:D_SMA")
    )
    (path
      (reference "J1") (unit 1) (value "Conn_01x03_Male") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical")
    )
    (path
      (reference "L1") (unit 1) (value "10uH 2A") (footprint "Inductor_SMD:L_Taiyo-Yuden_NR-50xx")
    )
    (path
      (reference "R1") (unit 1) (value "220k") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R2") (unit 1) (value "68k") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R3") (unit 1) (value "110k") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R4") (unit 1) (value "20k") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "U1") (unit 1) (value "AP63200WU") (footprint "Package_TO_SOT_SMD:TSOT-23-6")
    )
  )
)
